Back to Contents

# Specifications

- Intel(R) WiMAX/WiFi Link 5350
- Intel(R) WiMAX/WiFi Link 5150
- Intel(R) WiFi Link 5300
- Intel(R) WiFi Link 5100
- Intel(R) Wireless WiFi Link 4965AGN
- Intel(R) Wireless WiFi Link 4965AG_
- Intel(R) PRO/Wireless 3945ABG Network Connection
- Intel(R) PRO/Wireless 3945BG Network Connection
- Intel(R) PRO/Wireless 2915ABG Network Connection
- Intel(R) PRO/Wireless 2200BG Network Connection

## Intel(R) WiFi Link 5150 and Intel(R) WiFi Link 5350

WiFi / WiMAX
Form Factor | PCI Express* Mini Card and Half-Mini Card
SKUs | Intel® WiMAX/WiFi Link 5350 - 3x3 MC Intel® WiMAX/WiFi Link 5150 - 1X2 MC/HMC
Dimensions | Mini Card: Width 20 in x Length 1.18 in x Height 0.18 in (50.80 mm x 30 mm x 4.5 mm) Half-Mini Card: Width 1.049 in x Length 1.18 in x Height 0.18 in (26.64 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
Connector Interface | 53-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 90% non-condensing (at temperatures of 25 ºC to 35 ºC)
WiFi
Frequency Modulation | 5 GHz (802.11a/n) | 2.4 GHz (802.11b/g/n)
Frequency band | 5.15 GHz - 5.85 GHz (dependent on country) | 2.41-2.474 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | 4 to 12 (dependent on country) | Channel 1-11 (US only) Channel 1-13 (Japan, Europe)
IEEE 802.11n Data Rates | Intel(R) WiFi Link 5350 450, 405, 360, 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2 Mbps
Intel(R) WiFi Link 5150 300, 270, 243, 240, 180, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2 Mbps
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
WiFi General
Operating Systems | Microsoft Windows XP* (32 and 64 bit) and Windows Vista* (32 and 64 bit)
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, 802.11a, 802.11h, 802.11d, WPA-Personal, WPA-Enterprise, WPA2-Personal, WPA2-Enterprise, WMM, WMM Power Save, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
WLAN Standard | IEEE 802.11g, 802.11b, 802.11a, 802.11n
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, 802.1X: EAP-SIM, LEAP, PEAP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Encryption | AES-CCMP 128-bit, WEP 128-bit and 64-bit, CKIP, TKIP
Product Safety | UL, C-UL, CB (IEC 60590)
WiMAX
Frequency band | 2.5-2.7 GHz (3A Profile)
Modulation | UL - QPSK, 16 QAM DL - QPSK, 16 QAM, 64 QAM
Wireless Medium | Duplex mode: TDD operations | Scalable OFDMA (SOFDMA): 512 and 1024 FFT
sub-carrier permutation: PUSC | Channel bandwidths: 5 MHz and 10 MHz
WiMAX Network Release Feature set | SPWG/NWG Release 1.0 SPWG/NWG Release 1.5
Rate Performance (OTA performance 10MHz channel) | 10 Mbps DL and 4 Mbps UL @ peak rate
RF Transmitter Output Power | Compliance with Power class 2
WiMAX General
Operating Systems | Microsoft Windows XP* ,Vista*
Standard Compliance | 802.16e-2005 Corrigenda 2 (D4)
WiMAX System Profile Feature set | Mobile WiMAX release 1, Wave II Profile 3A
Security | Key Management Protocol (PKMv2)
Encryption | 128bit CCMP (Counter-Mode/CBC-MAC) based on AES encryption

## Intel(R) WiFi Link 5300 and Intel(R) WiFi Link 5100

Form Factor | PCI Express* Full-Mini Card and Half-Mini Card
Dimensions | Full-Mini Card: Width 2.00 in x Length 1.18 in x Height 0.18 in (50.95 mm x 30 mm x 4.5 mm) Half-Mini Card: Width 1.049 in x Length 1.18 in x Height 0.18 in (26.64 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
Connector Interface | 52-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 95% non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5 GHz (802.11a/n) | 2.4 GHz (802.11b/g/n)
Frequency band | 5.15 GHz - 5.85 GHz (dependent on country) | 2.400 - 2.4835 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | 4 to 12 (dependent on country) | Channel 1-11 (US only) Channel 1-13 (Japan, Europe)
IEEE 802.11n Data Rates | Intel(R) WiFi Link 5300 450, 405, 360, 300, 270, 243, 240, 216.7, 195, 180, 173.3, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2 Mbps
Intel(R) WiFi Link 5100 300, 270, 243, 240, 180, 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2 Mbps
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
General
Operating Systems | Microsoft Windows XP* (32 and 64 bit) and Windows Vista* (32 and 64 bit).
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, 802.11a, 802.11h, 802.11d, WPA-Personal, WPA-Enterprise, WPA2-Personal, WPA2-Enterprise, WMM, WMM Power Save, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
WLAN Standard | IEEE 802.11g, 802.11b, 802.11a, 802.11n
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit; 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Product Safety | UL, C-UL, CB (IEC 60590)

## Intel(R) Wireless WiFi Link 4965AGN

Form Factor | PCI Express* Mini Card
Dimensions | Width 2.00 in x Length 1.18 in x Height 0.18 in (50.95 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
Connector Interface | 52-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 95% non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5 GHz (802.11a/n) | 2.4 GHz (802.11b/g/n)
Frequency band | 5.15 GHz - 5.85 GHz (dependent on country) | 2.400 - 2.4835 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | 4 to 12 (dependent on country) | Channel 1-11 (US only) Channel 1-13 (Japan, Europe)
IEEE 802.11n Data Rates | Rx: 300, 270, 243, 240, 180 Rx/Tx: 150, 144, 135, 130, 120, 117, 115.5, 90, 86.667, 72.2, 65, 60, 57.8, 45, 43.3, 30, 28.9, 21.7, 15, 14.4, 7.2
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
General
Operating Systems | Microsoft Windows XP* (32 and 64 bit) and Windows Vista* (32 and 64 bit).
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, 802.11a, 802.11h, 802.11d, WPA-Personal, WPA-Enterprise, WPA2-Personal, WPA2-Enterprise, WMM, WMM Power Save, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
WLAN Standard | IEEE 802.11g, 802.11b, 802.11a, 802.11n
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit; 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Product Safety | UL, C-UL, CB (IEC 60590)

## Intel(R) Wireless WiFi Link 4965AG_

This is a version of Intel Wireless WiFi 4965AGN with 8-2.11n capabilities disabled. 802.11n refers to: IEEE P802.11n / D2.0 Draft Amendment to STANDARD [FOR] Information Technology-Telecommunications and information exchange between systems-Local and Metropolitan networks-Specific requirements-Part 11: Wireless LAN Medium Access Control (MAC) and Physical Layer (PHY) specifications: Enhancements for Higher Throughput.

Form Factor | PCI Express Mini Card
Dimensions | Width 2.00 in x Length 1.18 in x Height 0.18 in (50.95 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Antenna Diversity | On-board diversity
Connector Interface | 52-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50% to 95% non-condensing (at temperatures of 25 ºC to 35 ºC)
Frequency Modulation | 5 GHz (802.11a) | 2.4 GHz (802.11b/g)
Frequency band | 5.15 GHz - 5.85 GHz (dependent on country) | 2.400 - 2.4835 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | 4 to 12 (dependent on country) | Channel 1-11 (US only) Channel 1-13 (Japan, Europe)
IEEE 802.11a Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps
IEEE 802.11b Data Rates | 11, 5.5, 2, 1 Mbps
General
Operating Systems | Microsoft Windows XP (32 and 64 bit), and Windows Vista (32 and 64 bit)
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, 802.11a, WPA, WPA2, WMM, EAP-SIM
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
WLAN Standard | IEEE 802.11g, 802.11b, 802.11a
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit; 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Product Safety | UL, C-UL, CB (IEC 60590)

## Intel(R) PRO/Wireless 3945ABG Network Connection

Form Factor | PCI Express Mini Card
Dimensions | Width 2.00 in x Length 1.18 in x Height 0.18 in (50.95 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Dual Diversity Antenna | On-board dual diversity switching
Connector Interface | 52-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50 to 92% non-condensing (at temperatures of 25 ºC to 55 ºC)
Frequency Modulation | 5 GHz (802.11a) | 2.4 GHz (802.11b/g)
Frequency band | 5.15 GHz - 5.85 GHz | 2.400 - 2.4835 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | 4 to 12 non-overlapping, dependent on country | Channel 1-11 (US only) Channel 1-13 (Japan, Europe)
Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps | 11, 5.5, 2, 1 Mbps
General
Operating Systems | Microsoft Windows XP and Windows Vista
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, 802.11a, 802.11h, 802.11d, WPA-Personal, WPA-Enterprise, WPA2-Personal, WPA2-Enterprise, WMM, WMM Power Save, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
WLAN Standard | IEEE 802.11g, 802.11b, 802.11a
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit; 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Product Safety | UL, C-UL, CB (IEC 60590)

## Intel(R) PRO/Wireless 3945BG Network Connection

Form Factor | PCI Express Mini Card
Dimensions | Width 2.00 in x Length 1.18 in x Height 0.18 in (50.95 mm x 30 mm x 4.5 mm)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Dual Diversity Antenna | On-board dual diversity switching
Connector Interface | 52-pin Mini Card edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +80 degrees Celsius
Humidity | 50 to 92% non-condensing (at temperatures of 25 ºC to 55 ºC)
Frequency Modulation | 2.4 GHz (802.11b/g)
Frequency band | 2.400 - 2.4835 GHz (dependent on country)
Modulation | CCK, DQPSK, DBPSK
Wireless Medium | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | Channel 1-11 (US only) Channel 1-13 (Japan, Europe)
IEEE 802.11g Data Rates | 54, 48, 36, 24, 18, 12, 9, 6, 5.5, 2, 1 Mbps
IEEE 802.11g Data Rates | 11, 5.5, 2, 1 Mbps
General
Operating Systems | Microsoft Windows XP and Windows Vista
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, WPA, WPA2, WMM, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v4.0
WLAN Standard | IEEE 802.11g, 802.11b
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit; 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Product Safety | UL, C-UL, CB (IEC 60590)

## Intel(R) PRO/Wireless 2915ABG Network Connection

Form Factor | Mini PCI Type 3A
Dimensions | Width 2.85 in x Length 1.75 in x Height 0.20 in (72.39 mm x 44.54 mm x 5.08 mm)
Weight | 0.7 oz. (12.90 g.)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Dual Diversity Antenna | On-board dual diversity switching
Connector Interface | 124-pin SO-DIMM edge connector
Voltage | 3.3 Volt
Operating Temperature | 0 to +70 degrees Celsius
Humidity | 50 to 85% non-condensing
Frequency Modulation | 5 GHz (802.11a) | 2.4 GHz (802.11b/g)
Frequency band | 5.15 GHz - 5.85 GHz | 2.400 - 2.472 GHz (dependent on country)
Modulation | BPSK, QPSK, 16 QAM, 64 QAM | CCK, DQPSK, DBPSK
Wireless Medium | 5 GHz UNII: Orthogonal Frequency Division Multiplexing (OFDM) | 2.4 GHz ISM: Orthogonal Frequency Division Multiplexing (OFDM)
Channels | 4 to 12 non-overlapping, dependent on country | Channel 1-11 (US only) Channel 1-13 (Japan, Europe)
Data Rates | 54, 48, 36, 24, 18, 12, 9, 6 Mbps | 11, 5.5, 2, 1 Mbps
General
Operating Systems | Microsoft Windows XP and Windows Vista
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, 802.11a, WPA, WPA2, WMM, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v3.0
WLAN Standard | IEEE 802.11g, 802.11b, 802.11a
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA-Personal, WPA2-Personal, WPA-Enterprise, WPA2-Enterprise, AES-CCMP 128-bit, WEP 128-bit and 64-bit. 802.1X: EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Product Safety | UL, C-UL, CB (IEC 60590)

## Intel(R) PRO/Wireless 2200BG Network Connection

Form Factor | Mini PCI Type 3B
Dimensions | Width 2.34 in x Length 1.75 in x Height 0.20 in (59.45 mm x 44.45 mm x 5 mm)
Weight | 0.7 oz. (12.90 g.)
Antenna Interface Connector | Hirose U.FL-R-SMT mates with cable connector U.FL-LP-066
Dual Diversity Antenna | On-board dual diversity switching
Connector Interface | 124-pin mini PCI edge connector
Voltage | 3.3 V
Operating Temperature | 0 to +70 degrees Celsius
Humidity | 50 to 85% non-condensing
Frequency Modulation | OFDM with BPSK, QPSK, 16QAM, 64QAM, DBPSK, DQPSK, CCK
Frequency band | 2.400 - 2.472 GHz (US) 2.400 - 2.4835 GHz (Japan) 2.400 - 2.4835 GHz (Europe ETSI)
Modulation | OFDM with BPSK, QPSK, 16QAM, 64QAM, DBPSK, DQPSK, CCK
Channels | Full 14 channel support
Data Rates | 1, 2, 5.5, 6, 9, 11, 12, 18, 24, 36, 48 and 54 Mbps
General
Operating Systems | Microsoft Windows XP and Windows Vista
Wi-Fi Alliance* certification | Wi-Fi* certification for 802.11b, 802.11g, WPA, WPA2, WMM, EAP-SIM, LEAP, PEAP, TKIP, EAP-FAST, EAP-TLS, EAP-TTLS, EAP-AKA
Cisco Compatible Extensions certification | Cisco Compatible Extensions, v2.0
WLAN Standard | IEEE 802.11g and 802.11b
Architecture | Infrastructure or ad hoc (peer-to-peer) operating modes
Security | WPA, LEAP, PEAP, TKIP, EAP-TLS, EAP-TTLS, AES (128-bit), WEP 128-bit and 64-bit.
Product Safety | UL, C-UL, CB (IEC 60590)

Back to Top

Back to Contents

Trademarks and Disclaimers